**TiMotion Sit-Stand Electric Desk**

|  |  |
| --- | --- |
| An ergonomic, height adjustable sit-stand electric desk with minimal assembly.    Capabilities   * Variable desktop sizes available (see options) * Desktop thickness = 25mm * Frame width range = 1050-1850mm * Frame height range = 620-1275mm * Height adjustment speed = 40mm/sec * Noise level = 39dB * Standby power = <0.1W * 100kg maximum weight load * Minor assembly required | A versatile and ergonomic electric desk offering flexible height adjustment, easy to assemble with the partially pre-assembled frame (assembly time takes less than 6 minutes).  The TiMotion Sit-Stand Electric Desk Frame and Desktop is the ideal solution for creating an ergonomic sit-stand working environment. Features a high-class digital control box with memory buttons, USB charger, and a built-in anti-collision sensor.  Z:\Images\Products_current\TABLES and DESKS\TiMotion\TDH18P_02 memory 3.png  Features   * Dual motor * Electric height adjustability * Three step actuators * Low standby power and low noise level * Lockable height adjustment * Steel construction provides high strength and stability * Pre-assembled frame kit * Upper and lower height limit settings * Lock/unlock height adjustment * Built in anti-collision sensor control box (t-touch) * USB x 2 charger in control box * Memory settings   Options   * Black or white desk frame colour. * Variable sizes of white desktops available: * 1200 mm x 700 mm * 1500 mm x 750 mm * 1500 mm x 850 mm * 2100 mm x 800 mm * Extended warranty options. |